A black and white logo

Description automatically generated

EMBARGOED UNTIL JANUARY 22 AT 9:00 A.M. ET

**TRULLI AUDIO LAUNCHES NEW PRO AUDIO SUBWOOFER SYSTEM AT THE NAMM SHOW**

**Trulli Audio’s Bass50 System Represents a New Way to Deploy Commercial Audio.**

**MUNDELEIN, IL, January 22, 2026** – Today at The NAMM Show, Trulli Audio announced the world’s first professional-grade, battery-powered subwoofer system, representing a new way to deploy audio in commercial applications. In an industry first, the Trulli Bass50 System delivers high-output bass, achieving low-end accuracy commensurate with wired systems, via an audio solution that’s modular design allows it to scale from 50 to 5,000-person environments, without pulling power from the grid.

“For too long, commercial audio professionals have only been able to achieve premium sound though wired power and all the equipment, time and labor that comes with it,” said Len Foxman, Trulli Audio Founder and CEO. “The Trulli Bass50 System delivers real ‘low-end bass,’ can be set up in minutes, and can be optimized for nearly any environment.”

**Bass For Any Environment, No Sacrifices**

The Trulli Bass50 System is a one box rig that provides full impact bass without wall power, a generator, or installation. It was designed to help audio professionals quickly deploy premium audio setups in any environment. The heart of the system is the Trulli Bass50 Subwoofer, which contains an amp, DSP, battery, wireless receiver, and interface – all in one. Through Trulli’s mobile app, audio professionals can adjust and save settings like delay and crossover, including the high-pass filter, among others. The app also provides a series of preset audio profiles, optimized for different settings.

For further customization, the Trulli Bass50 System is equipped with wired and wireless connectivity options including a 3.5mm balanced Trip-Ring-Sleeve (TRS), USB-C digital audio input/outputs and SKAA wireless technology. This connectivity also enables users to modularly stack Trulli Bass50 systems together for larger venues.

A single Trulli Bass50 System includes:

* **Trulli Bass50 Subwoofer** – Incorporates the features noted above, as well as a replaceable, rechargeable battery with 5–10-hour life at full volume (EDM extreme music genre) that charges from 0-100% in 2.5 hours. It also sports a tough exterior that protects against the elements.
* **Trulli Universal Port** – A detachable enclosure that amplifies sound by up to 10 additional dB.
* **Bass50 Pole Plate** – M20 threaded pole mount for secure speaker placement setups.
* **Trulli Speaker Poles** – One-foot and three-foot poles for mounting satellite speakers.
* **Top-Speaker Compatibility** – Connectivity options that allow it to connect with nearly any top speaker including trusted brands like Bose Pro, QSC, Electro-Voice, PK Sound and more.

As a holistic commercial system in one package, the Trulli Bass50 System reduces the need for labor-heavy equipment and wires that can create tripping hazards or need to be hidden.

**Reinvented Speaker Driver**

All Trulli Subwoofers deliver accurate bass thanks to the use of our patented, award-winning ThinDriver® Technology, which helps them deliver more power at a fraction of the size (and air volume) compared to conventional speakers. The TD10S Driver in the Trulli Bass50 System can handle 600 Watts of continuous power, peaking at just over 1,000W and delivers up to 122 dB (131 dB with the Trulli Universal Port). It has a frequency range from 20Hz to 225Hz (30Hz to 80Hz with the Trulli Universal Port).

Trulli Audio has a suite of subwoofer drivers featuring ThinDriver® Technology – all designed for custom integrators. Each driver delivers premium performance in a minimalist profile, enabling cleaner, more practical builds. The portfolio includes:

* **TD19S 2000W and TD19S 5000W** – 19-inch subwoofer drivers with 4-inch mounting depth that can handle 2,000W of continuous power, and 6-inch mounting depth that can handle of continuous power 5,000W, respectively.
* **TD10S** – A 10-inch subwoofer driver with a 2.7-inch mounting depth that can handle 600W of continuous power.
* **TD6.5S** – A 6.5-inch subwoofer driver, with a 2.2-inch mounting depth, that can handle 300W of continuous power.

Trulli Audio’s full commercial portfolio is on display at The NAMM Show (Anaheim Convention Center, North 253A — Meeting Room 18816). For more information about Trulli Audio’s presence at the show and products, please visit [TrulliAudio.com](https://trulliaudio.com/). To become an authorized dealer, please visit [here](https://trulliaudio.com/pages/wholesale-application-authorized-dealer).

**About Trulli Audio**

Trulli Audio is an independent audio company based in Mundelein, IL. Founded by Len Foxman in 2016, Trulli’s mission to help music lovers fully experience the music they love without compromise, anywhere and everywhere they want superior sound. The company was born from Len’s lifelong love of jazz, matched with his extensive engineering credentials as long-time leader and president of Eagle Test Systems, which was acquired by Teradyne in 2008.

**Media Contact**

Jordan Neuhauser

847-366-4926

Jordan@TrulliAudio.com